
[Application_Title]
Title	=	"Uart Utility"
<END>

[Tab_Options]
Tab_Fifo_Levels	=	"Fifo"
Tab_Baudrate_Mapping	=	"Baud rates"
Tab_Line_Driver_Control	=	"Line drivers"
Tab_About	=	"About"
<END>

[Crystal_Frequency]
Show_Autodetect	=	"False"
<END>

[Fifo_Levels]
Tx_Interrupt_Level_Min	=	"1"
Tx_Interrupt_Level_Max	=	"127"
Rx_Interrupt_Level_Min	=	"1"
Rx_Interrupt_Level_Max	=	"127"
Flow_Control_On_Level_Min	=	"1"
Flow_Control_On_Level_Max	=	"127"
Flow_Control_Off_Level_Min	=	"1"
Flow_Control_Off_Level_Max	=	"127"
Transmit_Interrupt_Trigger_Level	=	"4"
Receive_Interrupt_Trigger_Level	=	"100"
Flow_On_Level	=	"16"
Flow_Off_Level	=	"112"
<END>

[Baudrate_Mapping]
<END>

[Line_Driver_Control]
Type	=	"No Control (RS232)"
<END>

[About]
Information	=	"\r\nOxford Semiconductor\r\nPCIe UART Driver\r\nwww.oxsemi.com"
ShowLogo	=	"False"
<END>
