______________________________________________________________________________

Windows CE 5.0 UART Configuration utility for PCI Express Devices
Copyright (C) 2008-2009 Oxford Semiconductor Inc.
______________________________________________________________________________

________________________________________

SUART - UART Configuration utility notes
________________________________________

This utility allows configuration of UART ports supported by this driver for
PCI Express devices. It provides a user interface to allow the end user
to modify features such as baud rate remapping, FIFO trigger levels etc.

Its content and appearance can be customised and branded by the Oxide
Branding utility (V3.0 or later).

For more notes on installation and use refer to Suart.doc
