CECInfo
(
	Name ( "PCIE950" )
	CECVersion ( 5.00 )
	GUID ( {BD43BA3D-B66A-4159-9CEE-C313E41DA388} )
)
ComponentType
(
	Name ( "Uarts" )
	GUID ( {55E508DA-C388-48B1-9C1E-7CDC7EF83DDD} )
	Group ( "\device drivers\serial" )
	Vendor ( "OEM" )
	MaxResolvedImpsAllowed( 999 )
	Implementations
	(
		Implementation
		(
			Name ( "pcie950" )
			GUID ( {0A613EEA-EC2E-4B1E-8D60-9B12F16545CD} )
			Version ( "2.0.0.2" )
			Locale ( 0409 )
			Vendor ( "OEM" )
			Date ( "12/01/2009" )
			SizeIsCPUDependent( 1 )
			BuildMethods
			(
				BuildMethod
				(
					GUID ( {083F3261-15F5-4716-B961-24B07F0C9F22} )
					Step ( CESYSGEN )
					CPU ( "ARMV4I" )
					CPU ( "x86" )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\OXSEMI\UARTS\isrpcie950\ISRpcie950.pbpxml" )' )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\OXSEMI\UARTS\mddpcie950\MDDpcie950.pbpxml" )' )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\OXSEMI\UARTS\pddpcie950\pddpcie950.pbpxml" )' )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\OXSEMI\UARTS\serpcie950\serpcie950.pbpxml" )' )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\OXSEMI\UARTS\compcie950\compcie950.pbpxml" )' )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\OXSEMI\UARTS\buspcie950\buspcie950.pbpxml" )' )
				)
			)
		)
	)
)
