# Marvell FastLinQ Edge Network Adapter Windows Driver
Aug 10, 2021

##v3.1.3.0
_Date 05.07.2021_
* Merged the changes from dev-release-3.0.x
* Added power management registry entry
* Modify ASUS Device Description for model XG-C100C
* Patch for WOL Issue

## v3.1.2.0
_Date 02.06.2021_
* Fixed NDISTest failures introduced with 3.1.0.0
* Logging linkstate at every boot-up
* 1c_OIDSwmi fails due to DASH status indication
* Driver updated to support Antigua DeviceIDs
* SleepOnDisconnect (D3D) Removed
* Add HWID for Lenovo AQC113C
* Add HWID for GigaByte-GC-AQC113C
* Added TODO on minor issues seen after merge
* Dirty wake with S3 and S4
* Added HWID for ASROCK-Z690

## v3.1.1.0
_Date 28.04.2021_
* Fixed NDISTest failures introduced in previous build 

## v3.1.0.0
_Date 22.04.2021_
* Added DASH support (integrated from 2.x branch)
* Added Service Mode support (from 2.x branch)
* Merged miscellaneous minor fixes and improvements from v2.x

##v3.0.21.0
_Date 29.06.2021_
* Modify ASUS Device Description for model XG-C100C.

##v3.0.20.0
_Date 09.06.2021_
* Driver updated to support Antigua DeviceIDs
* SleepOnDisconnect (D3D) Removed
* Logging linkstate at every boot-up
* Add HWID for Lenovo AQC113C
* Add HWID for GigaByte-GC-AQC113C
* Dirty wake with S3 and S4
* Added HWID for ASROCK-Z690 

## v3.0.19.0
_Date 22.01.2021_
* Removed unsupported RSS IPv6 extension header capability
* Removed unsupported half duplex speeds
* Disable DeviceSleepOnDisconnect by default
* Correct Hardware IDs for AQC113-based Asus NIC
* Enabled WakeFromPowerOff for AQC113

## v3.0.18.0
_Date 18.11.2020_
* Added Hardware IDs for AQC113-based Asus NIC
* Windows 8/8.1: enable PM by default for AQC113 (HCK requirement)
* Fixed RSC offload configuration (HLK test failure)
* Added workaround for OffloadLSO test failure in HLK 19041

## v3.0.17.0
_Date 12.10.2020_
* Security checks for secure AQC113 parts

## v3.0.16.0
_Date 31.08.2020_
* Support for Antigua B0 counters
* Additional HWIDs for Antigua
* Advertise 2.5G/5G NBase-T speeds along with 2.5/5G Base-T
* Add logging of 10Mbps link speed to system log.
* Fix reporting DeviceSleepOnDisconnect capability on Atlantic
* Fix RSC & Hyper-V vSwitch problem 


## v3.0.15.0
_Date 09.06.2020_
* Low Power on Media Disconnect
* Init-time instructions (as part of Low Power on Disconnect)
* Conformance to latest filtering spec: don't touch multicast filter
* Enable EEE for AQC113 family
* Fix TX stuck recovery logic
* Fixes & improvements for RSS logic for AQC107/AQC113
* Fixes D0->D3 state transition: drain transmit before disable interrupts

## v3.0.14.0
_Date 05.05.2020_
* Filtering infrastructure
* Dynamic interrupt resources allocation
* Separate trace flag for firmware layer
* Enable EEE at 1G link speed for AQC111C/AQC112C 
* Improve RX checksum offload workaround for AQC107
* Fix security checks on AQC107
* Remove auto-generation of MAC address
* Tidy up code

## v3.0.13.0
_Date 27.03.2020_
* Wake Reason Indications
* Provide firmware with the current MAC address
* WMI interface (not compatible with 2.x driver)
* Cable Diagnostics
* Changes for NDISTest compatibility
* Minor misc fixes and improvements

## v3.0.12.0
_Date 06.03.2020_
* Wake on ping behavior with ARP offload
* Update reset sequence
* Cleanup HAL

## v3.0.11.0
_Date 18.02.2020_
* Fixes for NDISTest
* Rework internal link parameters
* Update CI
* Update non-FF register to `0x1c`

## v3.0.10.0
_Date 05.02.2020_
* Set max frame length according to “Jumbo Packet” driver setting
* Add thermal shutdown support
* Add downshift support
* Link interrupt support
* Rework internal adapter state transitions

## v3.0.9.0
_Date 17.01.2020_
* Fix setting of packet filters for all multicast
* Fix setting of PFC
* Use standardized INF keywords for speed & duplex
* Introduce support for 10Mbps link speed
* Introduce support for half duplex

## v3.0.8.0: Alpha driver v3.0.8.0 for AQC113 famil
_Date 09.01.2020_
* Basic backward compatibility with AQC100/AQC107/AQC108
* Fixes for RSS multi-group
* Reworked interrupts logic
* Other minor fixes for AQC113 family

